Install.txt
-------------------------------------------------------------------------------
Optical Mark Reader USB Device Driver
                                     Copyright(C) 2002-2009 SEKONIC CORPORATION
-------------------------------------------------------------------------------


Procedures for installing the USB device driver in Windows 98
------------------------
*:Operation by this OS is not guaranteed.

1) Insert the CD-ROM to the host, and connect the OMR scanner with the host 
   by using the USB cable.
2) 'Found New Hardware Wizard' is automatically activated, and 'Optical Mark 
   Reader' is detected. Click 'Next'.
3) Select 'Search for the best driver for your device.' by 'What do you want 
   Windows to do?'. Click 'Next'.
4) Select 'Specify a location' first, and select '\Driver' of the directory on 
   CD-ROM drive. Click 'Next'.
5) 'USB SEKONIC Optical Mark Reader Device' is detected. Click 'Next'.
6) Copy of the USB driver is made from the CD-ROM, and 'USB SEKONIC Optical 
   Mark Reader Device' is displayed. Click 'Finish'.

  Installation is finished on the above procedures.



Procedures for installing the USB device driver in Windows Me
------------------------
*:Operation by this OS is not guaranteed.

1) Insert the CD-ROM to the host, and connect the OMR scanner with the host by 
   using the USB cable.
2) 'Add New Hardware' is automatically activated, and 'Optical Mark Reader' is 
   detected. Select 'Specify the location of the driver' and click 'Next'.
3) Select 'Search for the best driver for your device' and 'Specify a location' 
   next, and then select '\Driver' of the directory on CD-ROM drive. 
   Click 'Next'.
4) The file is detected and 'USB SEKONIC Optical Mark Reader Device' is 
   displayed. 
   The file is named and displayed as '\Driver\SkSr6500.inf'. Click 'Next'.
   Note: All other check boxes should be deleted, and select 'Specify a 
   location' ONLY.
5) Copy of the USB driver is made from the CD-ROM, and 'USB SEKONIC Optical 
   Mark Reader Device' is displayed. Click 'finish'.

  Installation is finished on the above procedures.



Procedures for installing the USB device driver in Windows 2000
------------------------

Note: Log-on by Administrator.

1) Insert the CD-ROM to the host, and connect the OMR scanner with the host by 
   using the USB cable.
2) 'Found New Hardware Wizard' is automatically activated.
3) 'Optical Mark Reader' is detected. Select 'Search for a suitable driver for 
   my device.' by 'What do you want the wizard?'. Click 'Next'.
4) Select 'Specify a location', and click 'Next'.
5) Select '\Driver\Win2k' by 'Insert the manufacturer's installation disk into 
   the drive selected , and then click OK', Click 'OK'.
   Note: All other check boxes should be deleted, and select 'Specify a 
   location' ONLY.
6) The file is detected and 'USB SEKONIC Optical Mark Reader Device' is 
   displayed. The file is named and displayed as '\Driver\SkSr6500.inf'. 
   Click 'Next'.
7) Copy of the USB driver is made from the CD-ROM, and 'USB SEKONIC Optical 
   Mark Reader Device' is displayed. Click 'Finish'.

  Installation is finished on the above procedures.



Procedures for installing the USB device driver in Windows XP
------------------------

Note: Log-on by Administrator.

1) Insert the CD-ROM to the host, and connect the OMR scanner with the host by 
   using the USB cable.
2) 'Found New Hardware Wizard' is automatically activated, and 'Optical Mark 
   Reader' is detected. Select 'Install from a list or specific location' by 
   'What do you want the wizard to do?'. Click 'Next'.
3) Select 'Please choose your search and installation options.' and 'Search for 
   the best driver in these locations.' next and 'Include this location in the 
   search.' further, and then select '\Driver' of the directory on the CD-ROM 
   drive. Click 'Next'.
4) The file is detected and 'USB SEKONIC Optical Mark Reader Device' is 
   displayed.  Copy of the file is being made.
5) Copy of the USB driver is made from the CD-ROM, and 'USB SEKONIC Optical 
   Mark Reader Device' is displayed. Click 'Finish'.

  Installation is finished on the above procedures.



Procedures for installing the USB device driver in Windows Vista
------------------------

Note: Log-on by Administrator.

1) Insert the CD-ROM to the host, and connect the OMR scanner with the host by 
   using the USB cable.
2) 'Found New Hardware Wizard' is automatically activated.
   Select 'Locate and install driver software(recommended)'
   by 'Windows needs to install driver software for your'.
3) 'User Account Control'window is displayed.
   Click 'Continue'.
4) Select 'Don't search online' 
   by 'Allow Windows to search online for driver software for your?'.
5) 'Insert the disc that came with your' window is displayed.
   Click 'Next'.
6) 'Windows can't verify the publisher of this driver software' window is 
   displayed.  Click 'Install this driver software anyway'.
   Copy of the file is being made.
7) Copy of the USB driver is made from the CD-ROM, and 'SEKONIC SR-1800 Device' 
   is displayed. Click 'Close'.

  Installation is finished on the above procedures.



Microsoft and Windows are registered trademarks of Microsoft Corporation 
(U.S.A.) in the United States and other countries.
The other listed product names are registered trademarks or trademarks of 
Microsoft Corporation.
